Use Windows Device Manager to install driver for ZHW01-M3 USB<>COM adapter.

1. Open the Windows Start menu and select the Control Panel. Select System and Security and then open the Device Manager.
2. The device will be listed under "Other devices". In this example a 'USB2.0-Ser!' has been connected to the PC. Right-click on the device and select Update Driver Software... from the pop-up menu.
The Update Driver Software wizard will open.
3. Click Browse my computer for driver software to continue.
4. Click the Browse... button and select the folder \USB_driver\drv. Check Include subfolders, then click Next to proceed.
5. Windows will search the selected folder for the driver and when it has found it, the installation will proceed.
When the driver installation is complete, the final page of the Wizard will appear.
6. Click Close. It is now possible to connect to the ZHW01-M3 cnc pendant device. The newly installed device will be listed under "Ports (COM & LPT)" in the Device manager.




Для установки USB-драйвера для USB<>COM адаптера пульта ZHW01-M3 используйте диспетчер устройств Windows.

1. Отройте меню "Пуск" и выберите "Панель управления". Выберите категорию "Система и безопасность" и откройте Диспетчер Устройств.
2. Устройство вероятнее всего будет находиться в списке "Другие устройства". В случае с пультом ZHW01-M3 название подключенного USB<>COM переходника будет иметь вид 'USB2.0-Ser!'. Щелкните правой кнопкой мыши на этом устройстве и выберите "Обновить драйверы ..." из списка меню.
Откроется мастер обновления драйвера устройства.
3. Выберите вариант "Выполнить поиск драйверов на этом компьютере". 
4. С помощью кнопки "Обзор" укажите путь к папке с файлами драйверов \USB_driver\drv. Убедитесь, что установлена галочка "Включая вложенные папки". Нажмите "Далее".
5. ОС Windows будет искать требуемый для устройства драйвер в выбранной папке. Если драйвер будет найден, мастер перейдет к установке драйвера для устройства. После завершения установки драйвера откроется завершающая вкладка Мастера установки.
6. Нажмите "Закрыть". Теперь USB<>COM переходник пульта ZHW01-M3 подключен к системе и готов к использованию. Аналогичные новые пульты, подключенные к этому компьютеру будут отображаться в списке Порты (COM и LPT).